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 OTDR

Optical Time Domain Reflectometer (OTDR) acquires and analyses the information of backscattering and reflective light propagating in fiber, based on the light backscatter and Fresnel reflection principle, to get the length, loss, fault points, light return loss, connector loss and so on. It is an essential tool for optical cable construction, deployment and maintenance.

The DVP323 series is a high-performance portable OTDR presented in 2017. This series product adopts some new techniques such as touch screen and real-time analysis. The optimized interface makes operations more convenient. Meanwhile the OPM and VFL are standard accessories. It is the best tool for fiber construction, deployment and maintenance.

Features 

5 inch touch screen, 800×480 high dot array resolution

Compact structure design, lighter, thinner and smaller

Exceptional short distance performance; minimum 0.8m event dead zone; minimum 4m attenuation dead zone

Support 28dB to 36dB dynamic range of various application demands

Convenient and fast UE design

Support OPM and VFL 

Complete data interfaces such as LAN, USB and so on

SPECIFICATIONS 
	Model
	Wavelength(nm)
	Dynamic Range(dB)
	Event Dead Zone (m)
	Attenuation Dead Zone (m)

	DVP323
	1310±20/1550±20
	34/32
	<3m
	<25m

	Distance range(Km)
	5m-160km

	Pulse width(ns)
	5ns~20μs（5ns, 10ns, 20ns, 50ns, 100ns, 200ns, 500ns, 1μs, 2μs, 5μs, 10μs, 20μs）

	Measurement time
	user-defined(smart link),with real-time measurement function

	Distance accuracy(m)
	±（1m +0.001%×range + sampling resolution）

	Attenuation accuracy
	±0.05dB/dB

	Loss limit(dB)
	0.01dB

	Loss resolution(dB)
	0.001dB

	Sampling resolution(m)
	0.1m

	Sampling points
	128000

	Data storage
	3000 items


OTHER INDICATORS
	LCD type
	5 inch TFT colorized LCD

	Laser adapter
	FC/PC, SC/PC(option)

	Interface
	USB

	Battery
	built-in rechargeable Li-ion battery  charging time <4 hours working time >8 hours

	Power
	AC input : 100~240V , 600mA , 50/60Hz       DC output : 12.0V , 2A

	Operating temperature
	0℃～40℃

	storage temperature
	-20℃～70℃

	relative humidity
	<80%

	weight
	<1kg

	dimensions (mm)
	200*126*62mm
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