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DVP Optical Power Meter Series
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——Features
——
• High performance detector

• Stable and reliable 

• High sensitivity

• Multi-wave test

• Relative and absolute power display

• SMT, lightweight

• Power supply by battery

——Applications ——
• Fiber loss testing

• Cable building, inspecting and maintaining

• Fiber identification

• Fiber system experiment and testing

• CATV testing

• Optical transmitter adjusting test

——Specifications ——
	Model
	DVP-2001
	       DVP-2002

	Optical detector
	InGaAs
	InGaAs/Attenuation

	Wavelength
	850 nm、980nm、1300nm、1310nm、1480nm、1550nm、1625nm

	Dynamic range
	-70～+3dBm
	-40～+33dBm

	Accuracy
	±５％

	Display
	λ，mW，nW，uW，pW，dBm，dB

	Interface
	FC/Universal adaptor(2001A)
	FC/Universal adaptor(2002A）；

FC/ST/SC/MU/LC（2002B）

	Power Supply
	2 AA battery（battery life>100H）

	Storage environment
	-20～+55℃ 0～95%(no condensation ）
	-20～+55℃  0～95%（ no condensation ）      

	Storage environment
	-40～+70℃  0～95%（ no condensation ）

	Dimensions
	62mm×22mm×110mm

	Weight
	0.1Kg


