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DVP-740 Mini FTTx Fusion Splicer
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Features
                                               
Compact & Light weight

Applied for Fibers, Cables and SOC (splice- on connector)
Integrated Holder Design 
Fully Automatic, Semi-automatic and Manual Operation
Shockproof, Drop resistance
Power saving Function
4.3 inch Color LCD monitor

USB&DC interface
SPECIFICATIONS
	Applicable fibers
	SM, MM, DS, NZ-DS(G655), EDF, Bending Loss Insensitive fiber(G657), Pigtail, Drop cable and connector.


	Fiber cleaved length
	8-22mm

	Average splice loss
	0.02dB(SM)、0.01dB(MM)、0.04dB(DS)、0.04dB(NZDS)

	Return loss
	≥60dB

	Tension test
	2.0N(200gf)(Standard)

	Protection sleeve length
	20mm, 40mm, 60mm


	Splice Program
	5 groups of preset programs, 75 group of manual setting 

	Language

	English, Chinese, Russian, Spanish, Portuguese.

	Environment conditions
	-25～＋50℃ (operation temperature), 0～95%RH (humidity), 0～5000m (altitude)

	Storage environment
	-40～ +80℃ (temperature) , 0～95％RH (humidity)


	Power supply
	AC adaptor： 85～260V input voltage


Internal battery: 12V, 5.2Ah, up to 120 times of continuous splice and heat

	Dimensions/Weight
	142（D）×122（W）×138（H）mm/1.95kg


STANDARD PACKAGE
Fusion Splicer, Fiber Cleaver, Drop Cable Stripper, Connector holder, Heater Device for Connector, Spare Electrodes, Charger, Cooling Tray, Manual Instruction, Carry Box/ Bag.
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