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DVP-322 OTDR
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Features 

One-key operation, easy to operate                    

Smart portable OTDR, 4.3’TFT LCD display       
Firm, durable, shock-proof, moisture-proof 

Automatic trouble–shooting and calibration

 (VFL)Visual fault location function
Built-in lithium rechargeable battery, more than 8 hours working hours

Support USB and RJ45 interface, more convenient to manage files
Toolbox PC simulation software
SPECIFICATIONS 
	Model
	Wavelength(nm)
	Dynamic Range(dB)
	Event Dead Zone (m)
	Attenuation Dead Zone (m)

	DVP322
	1310±20/1550±20
	31/29
	<3m
	<25m

	Distance range(Km)
	5m-160km

	Pulse width(ns)
	5ns~20μs（5ns, 10ns, 20ns, 50ns, 100ns, 200ns, 500ns, 1μs, 2μs, 5μs, 10μs, 20μs）

	Measurement time
	user-defined(smart link),with real-time measurement function

	Distance accuracy(m)
	±（1m +0.001%×range + sampling resolution）

	Attenuation accuracy
	±0.05dB/dB

	Loss limit(dB)
	0.01dB

	Loss resolution(dB)
	0.001dB

	Sampling resolution(m)
	0.1m

	Sampling points
	128000

	Data storage
	3000 items


OTHER INDICATORS
	LCD type
	4.3 inch TFT colorized LCD

	Laser adapter
	FC/PC, SC/PC(option)

	Interface
	USB、RJ45

	Battery
	built-in rechargeable Li-ion battery  charging time <4 hours working time >8 hours

	Power
	AC/DC adapter  input AC90-240V ±10%  output DC12V

	Operating temperature
	0℃～40℃

	storage temperature
	-20℃～70℃

	relative humidity
	<80%

	weight
	<1kg

	dimensions (mm)
	200*126*62mm
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