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DVP-1660 Visual Fault Locator



—— Features ——
2.5mm universal connector
Operates either in CW or Pulsed
Constant output power 
Lower Battery warning
Long battery life 
Crash-proof and dust-proof design for laser head
Laser case ground design  prevents ESD damage
Burning testing to ensure the reliability.
Portable and rugged, easy to use
Guarantee to CE standards include EMC, EMI, ROHS

—— Specifications ——
	MOdel
	DVP1660

	 Output power
	1mW、3mW、5mW、10mW can be optional on customer request

	 Wavelength
	650

	 Emitter type
	FP-LD

	 Optical connector
	2.5mm Universal connector, 1.25mm connector

	 Operating model
	CW、2HZ

	Battery operating time
	65 hous/650nm@1mW

	 Power supply
	2 pcs of AA battery

	 Operating temperature（°C）
	-10~+45

	 Storage temperature（℃）
	-40~+70

	 Dimensions（mm）
	φ15*180

	Weight（g）
	120


DVP-1660 is specially designed for field personnel who need an efficient and economical tool for fiber tracing, fiber routing and continuity checking in an optical network during and after installation. It includes finding the breakpoint, poor connections, bending or cracking in fiber optic cables.Finding the faults of OTDR











